| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Cooling System > Water Temperature Control Assembly>Repair procedures |

Removal and Installation
1. | Loosen the drain plug, and drain the engine coolant. Remove the radiator cap to drain with speed.
2. | Disconnect the battery negative terminal.
3. | Remove the air cleaner assembly. (Refer to Intake and exhaust system - "Air Cleaner")
4. | Disconnect the water temperature sensor connector (A).
5. | Disconnect the radiator upper hose (B).
6. | Remove the heater hose (C).
7. | Disconnect the water hose (D).
8. | Remove the water temperature control assembly (B).
Tightening torque : 9.8 ~ 11.7N.m (1.0 ~ 1.2kgf.m, 7.2 ~ 8.7lb-ft)
9. | Install in the reverse order of removal.
Clean the surface of the water temperature control assembly before installing.