| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Rear Parking Assist System>Specifications |

Specification
Description | Specification
Ultrasonic sensor | Rated voltage | DC 12V
Detecting range | 11.8~47.2 in (300 ~ 1,200 mm)
Operating voltage | DC 8 ~ 10 V
Rated current | MAX. 20 mA
Operating temperature | -22°F~+176°F(-30°C ~ +80°C)
Preservation temperature | -40°F~+185°F(-40°C ~ +85°C)
Frequency | 48 ± 5 KHZ
Number of sensors | 4 EA (Right, Center-right, Center-left, Left)