| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Intake And Exhaust System > Intercooler Pipe & Hose>Repair procedures |

Removal and Installation
1. | Remove the air duct and air cleaner assembly. (Refer to Intake and Exhaust System - "Air Cleaner")
2. | Remove the intercooler outlet hose(A).
Tightening torque : 4.9 ~ 6.8N.m (0.5 ~ 0.7 kgf.m, 3.6 ~ 5.0 lb-ft)
3. | Remove the intercooler inlet hose & pipe(A).
Tightening torque Bolt : 19.6 ~ 26.4N.m (2.0 ~ 2.7 kgf.m, 14.4 ~ 19.5 lb-ft) Clamp : 4.9 ~ 6.8N.m (0.5 ~ 0.7 kgf.m, 3.6 ~ 5.0 lb-ft)
4. | Install in the reverse order of removal.
• | Match the marking part of hose and marking part of throttle body, compressor .
• | Match the pipe stopper and hose marking.
• | When the band part have been place on the top of position mark of hose, install to not exceed the mark.
• | Tighten until the torque control cap is released. If there is no the torque control cap, tighten as specified torque.