| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Hands Free System > Hands Free Mic>Repair procedures |

Inspection
1. | Disconnect the negative(-) battery terminal.
2. | Remove the roof trim. (Refer to the BD group - "Roof trim")
3. | Remove the handsfree mic (A) after disconnect the connector from roof top.
Be careful not to damage the roof trim when removing the hands free mic.
4. | Check the continuity of Mic between terminals.