| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Intake And Exhaust System > Intercooler>Repair procedures |

Removal and Installation
1. | Disconnect the battery negative terminal.
2. | Disconnect the boost pressure sensor connector(A) RCV solenoid valve connector(B) cooling fan controller connector(C).
3. | Disconnect the vacuum hose(D).
4. | Disconnect the intercooler outlet hose. (Refer to Intake and Exhaust System - "Intercooler pipe & hose")
5. | Disconnect the intercooler inlet hose. (Refer to Intake and Exhaust System - "Intercooler pipe & hose")
6. | Remove the radiator upper bracket(A).
7. | Disconnect the RCV hose(A) and then remove the intercooler(B).
8. | Install in the reverse order of removal.