| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Electrical System > General Information>Specifications |

Specification
Ignition System
Ignition Coil
Item | Specification
Primary Coil Resistance (Ω) | 0.79 ± 15％ [20°C (68°F)]
Secondary Coil Resistance (kΩ) | 7.0 ± 15％ [20°C (68°F)]
Spark plug
Item | Specification
Type | SILZKR6D8E
Gap | 0.7 ~ 0.8 mm (0.028 ~ 0.31 in.)
Condenser
Item | Specification
Capacitance (uF) | 0.47 [1KHz]
Insulation resistance (mΩ) | 1,000 [DC 500 V/1 Min]
Charging System
Alternator
Item | Specification
Rated voltage | 13.5V, 110A
Speed in use | 1,000 ~ 18,000 rpm
Voltage regulator | IC Regulator built-in type
Regulator Setting Voltage | External mode | Refer to below graph
Internal mode | 14.55 ± 0.3V
Temperature Gradient | External mode | 0 ± 3 mV / °C
Internal mode | -3.5 ± 2mV / °C
※ Regulator Setting Voltage (External mode) Battery
Item | Specification
Model type | CMF45L-DIN
Capacity [20 HR / 5HR] (AH) | 45 / 36
Cold Cranking Amperage (A) | 410 (SAE) / 330 (EN)
Reserve Capacity (Min) | 80
• | Model type description
• | Cold Cranking Ampere (CCA): Cold Cranking Amps is a rating used in the battery industry to define a battery's ability to start an engine in cold temperatures.
- | The rating is the number of amps a new, fully charged battery can deliver at -18 °C(-0.4 °F) for 30 seconds, while maintaining a voltage of at least 7.2 volts for a 12 volt battery.
- | The higher the CCA rating, the greater the starting power of the battery.
• | RESERVE CAPACITY (RC) : Reserve Capacity is a battery industry rating, defining a battery's ability to power a vehicle with an inoperative alternator or fan belt.
- | The rating is the number of minutes a battery at 26.7 °C(80 °F) can be discharged at 25 amps and maintain a voltage of 10.5 volts for a 12 volt battery.
- | The higher the reserve rating, the longer your vehicle can operate should your alternator or fan belt fail.
Starting System
Starter
Item | Specification
Rated voltage | 12 V, 0.9 kW
The number of pinion teeth | 10
Performance [No-load, 11.5 V] | Ampere | Max. 60 A
Speed | Min. 5,500 rpm
Tightening Torques
Item | N.m | kgf.m | lb-ft
Ignition coil installation bolt | 9.8 ~ 11.8 | 1.0 ~ 1.2 | 7.2 ~ 8.7
Spark plug installation | 14.7 ~ 24.5 | 1.5 ~ 2.5 | 10.9 ~ 18.1
Condenser & Hanger bracket installation nut | 18.6 ~ 23.5 | 1.9 ~ 2.4 | 13.7 ~ 17.4
Alternator installation bolt [12 mm (0.47 in.)] | 19.6 ~ 26.5 | 2.0 ~ 2.7 | 14.5 ~ 19.5
Alternator installation bolt [14 mm (0.55 in.)] | 29.4 ~ 41.2 | 3.0 ~ 4.2 | 21.7 ~ 30.4
Battery (+) terminal tightening nut | 7.8 ~ 9.8 | 0.8 ~ 1.0 | 5.2 ~ 8.7
Battery (-) terminal l tightening nut | 3.9 ~ 5.9 | 0.4 ~ 0.6 | 2.9 ~ 4.3
Battery mounting bracket bolt | 8.8 ~ 13.7 | 0.9 ~1.4 | 6.5 ~ 10.1
Battery tray installation bolt | 8.8 ~ 13.7 | 0.9 ~1.4 | 6.5 ~ 10.1
Battery sensor cable installation bolt | 29.4 ~ 31.4 | 3.0 ~ 3.2 | 21.7 ~ 23.1
Starter installation bolt | 49.0 ~ 63.7 | 5.0 ~ 6.5 | 36.2 ~ 47.0