| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Indicators And Gauges>Troubleshooting |

Troubleshooting
Symptom | Possible cause | Remedy
Tachometer does not operate | Cluster fuse (10A) blown | Check for short and replace fuse
CAN line faulty | Check the EMS
Tachometer faulty | Check tachometer
Wiring or ground faulty | Repair if necessary
Fuel gauge does not operate | Cluster fuse (10A) blown | Check for short and replace fuse
Fuel gauge faulty | Check gauge
Fuel sender faulty | Check fuel sender
Wiring or ground faulty | Repair if necessary
Low fuel warning lamp does not light up | Cluster fuse (10A) blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Fuel sender faulty | Check fuel sender
Wiring or ground faulty | Repair if necessary
Water temperature gauge does not operate | Cluster fuse (10A) blown | Check for short and replace fuse
Water temperature gauge faulty | Check gauge
Water temperature sender faulty | Check sender
CAN line faulty | Check the EMS
Wiring or ground faulty | Repair if necessary
Oil pressure warning lamp does not light up | Cluster fuse (10A) blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Oil pressure switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Parking brake warning lamp does not light up | Cluster fuse (10A) blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Brake fluid level warning switch faulty | Check switch
Parking brake switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
CAN line faulty | Check the TCS/ABS (EBD) Check the Smart Junction Box(SJB) (Parking brake/Brake oil switch)
Open door warning lamp and trunk warning lamp do not light up | Cluster fuse (10A) blown | Check for short and replace fuse
Bulb burned out | Replace bulb
CAN line faulty | Check the Smart Junction Box(SJB)
Door switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Speedometer does not operate | Vehicle speed sensor faulty | Check the vehicle speed sensor (M/T)
CAN line faulty | Check the EMS (A/T)
Seat belt warning lamp does not light up | Cluster fuse (10A) blown | Check for short and replace fuse
Bulb burned out | Replace bulb
CAN line faulty | Check the BCM
Seat belt switch faulty | Check switch
Wiring or ground faulty | Repair if necessary