| VELOSTER(FS) >2013 > G 1.6 T-GDI > Suspension System > Tire Pressure Monitoring System>General Information |

General Information
Specifications
Valve type | Snap in
Color | Case | Black
Label | White
CAN | LOW -Line
Frequency | 315 MHz
Pressure Warning standard | Rim size | RCP | Warning ON | Warning OFF
17” ,18” | 32 PSI(220 kPa) | 25 PSI(172 kPa) | 30PSI(206 kPa)
Component parts
1. | ECU Function
A. | Auto Learning
B. | Fail safe
C. | Logic Control
D. | RF (Radio Frequency) Receive
2. | WE’ sensor (Wheel Electronic sensor) Function
A. | Pressure, Temperature, Accelerometer Sensing
B. | RF (Radio Frequency) Transmit
3. | Display
A. | Equipped position -Cluster
B. | Warning system for air pressure - Warning lamp on(1 LED , Low-pressure tires can not be displayed)
C. | Shape warning lamp