| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Electrical System > Ignition System>Repair procedures |

On-vehicle Inspection
Inspect ignition coil assembly and Perform spark test
1. | Check for DTCs.
• | If a DTC is present, perform troubleshooting in accordance with the procedure for that DTC. (Refer to DTC guide)
2. | Check if sparks occur.
(1) | Remove the engine cover.
(2) | Remove the cylinder head center cover.
(3) | Remove the ignition coils.
(4) | Using a spark plug wrench, remove the spark plugs.
(5) | Disconnect the 4 injector connectors.
(6) | Ground the spark plug to the engine.
(7) | Check if sparks occur at each spark plug while engine is being cranked.
• | Do not crank the engine for more then 5 seonds.
3. | If sparks do not occur, perform the following test.
4. | Using a spark plug wrench, install spark plugs.
5. | Install the ignition coils.
6. | Install the cylinder head center cover and the engine cover.