| VELOSTER(FS) >2013 > G 1.6 T-GDI > Brake System > ESC(Electronic Stability Control) System>Schematic Diagrams |

Circuit Diagram - ESC (1)
Circuit Diagram - ESC (2)
Circuit Diagram - ESC (3)
Circuit Diagram - ESC (4)
ESC connector input/output
Connector Terminal | Specification | Remark
No | Description
29 | IGNITION1(+) | High level of wake up voltage : 4.5V < V < 16.0V Low level of wake up voltage : V < 2.4V Max. current : I < 50mA |
25 | POS. BATTERY 1.(SOLENOID) | Over voltage range : 17.0 ± 0.5V Operating voltage range : 10.0 ± 0.5V < V < 16.0 ± 0.5V Low voltage range : 7.0 ± 0.5V < V < 9.5 ± 0.5V Max. current : I < 40A Max. leakage current : I < 0.25mA |
1 | POS. BATTERY 2.(MOTOR) | Operating voltage range: 10.0 ± 0.5V < V < 16.0 ± 0.5V Rush current : I < 110A Max current : I < 40A Max leakage current : I < 0.25mA |
38 | GROUND | Rated current : I <550mA Max. current: I < 40A |
13 | PUMP MOTOR GROUND | Rush current : I < 110A Max current : I < 40A |
11 | SENSOR GROUND | Rated current : I <250mA |
4 | SENSOR POWER | Max current Capability : I < 250mA Max voltage : V_BAT1 -0.8V |
23 | BRAKE LIGHT SWITCH | Input voltage (Low) : V < 2.0V Input voltage (High) : V > 6.0V Max. Input current : I < 3mA (@12.8V) |
10 | ESC ON/OFF SWITCH
9 | BRAKE SWITCH
22 | PARKING BRAKE SWITCH | Input voltage (Low) : V < 2.0V Input voltage (High) : V > 6.0V Max input current : I < 5mA (@12.8V) |
28 | SENSOR FRONT RIGHT OUTPUT | External pull up resistance :1 KΩ < R Output duty : 50 ± 20% |
14 | CAN BUS LINE(LOW) | Max. Input current : I < 10mA |
26 | CAN BUS LINE(HIGH)
18 | SENSOR FRONT LEFT POWER | Output voltage : V_BAT1 -0.6V ~ V_BAT1 -1.1V Output current : Max 30mA |
34 | SENSOR FRONT RIGHT POWER
19 | SENSOR REAR LEFT POWER
33 | SENSOR REAR RIGHT POWER
31 | SENSOR FRONT LEFT SIGNAL | Input current LOW : 5.9 ~ 8.4mA Input current HIGH : 11.8 ~ 16.8mA Frequency range : 1 ~ 2,500Hz Input duty : 50 ± 10% |
21 | SENSOR FRONT RIGHT SIGNAL
32 | SENSOR REAR LEFT SIGNAL
20 | SENSOR REAR RIGHT SIGNAL
12 | CAN SENSOR LINE (HIGH) | Max. input current : I < 10mA |
24 | CAN SENSOR LINE (LOW)
8 | HAC RELAY DRIVE | Max. current : I < 180mA Max output voltage : V< 1.2V |
36 | HAC RELAY STATE MONITORING | Input voltage (Low) : V < 2V Input voltage (High) : V > 6V Max input current : I < 10mA (@12.8V) |