| VELOSTER(FS) >2013 > G 1.6 T-GDI > Manual Transaxle System > Manual Transaxle Control System > Back-up Lamp Switch>Repair procedures |

Inspection
1. | Disconnect the back up lamp switch connector (A).
2. | Check the continuity between no. 1 and 2 terminals of backup lamp switch. When the shift lever is in reverse, there should be continuity.
3. | If necessary, repair or replace the backup lamp switch.
Replacement
1. | Disconnect the back up lamp switch connector (A).
2. | Remove the back up lamp switch (A).
3. | Replace a new one and install the back up lamp switch.
Tightening torque: 29.4 ~ 34.3 N.m (3.0 ~ 3.5 kgf.m, 21.7 ~ 25.3 lb-ft)