| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Intake And Exhaust System > Air Cleaner>Repair procedures |

Removal and Installation
1. | Remove the engine cover.
2. | Disconnect the battery negative terminal.
3. | Remove the air duct and air cleaner assembly.
Tightening torque Hose clamp bolt: 2.9 ~ 4.9N.m (0.3 ~ 0.5kgf.m, 2.2 ~ 3.6lb-ft) Air cleaner assembly bolts: 7.8 ~ 9.8N.m (0.8 ~ 1.0kgf.m, 5.8 ~ 7.2lb-ft)
(1) | Remove the air duct(A).
(2) | Disconnect the breather hose (B), RCV hose (C) and air intake hose (D).
(3) | Remove the air cleaner assembly (E).
Hose clamp is fitted by matching from the hose stopper plate.
4. | Install in the reverse order of removal.