| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body (Interior and Exterior) > Seat & Power Seat > Rear Seat>Repair procedures |

Replacement
Rear Seat Assembly Replacement
1. | After loosening the mounting bolts, then remove the rear seat cushion (A).
Tightening torque : 16.7 ~ 25.5 N.m (1.7 ~ 2.6 kgf.m, 12.3 ~ 18.8 lb-ft)
2. | After loosening the mounting bolts, then remove the rear seat back (A).
Tightening torque : 16.7 ~ 25.5 N.m (1.7 ~ 2.6 kgf.m, 12.3 ~ 18.8 lb-ft)
3. | Installation is the reverse of removal.
Seat Back Cover Replacement [LH]
• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts your hands.
• | Put on gloves to protect your hands.
1. | Remove rear seat back assembly.
2. | Push the lock pin (B), remove the headrest (A).
3. | Remove the rear seat folding lever (A) after turning in the counter clock-wise direction.
4. | Remove the rear seat folding lever cover (B).
5. | After loosening the mounting screws, then remove the rear seat latch cover (A).
6. | Using a screwdriver or remover, remove the rear seat side bracket cover (A).
7. | Push the protecter (B) by the rear seat back panel (A).
8. | Using a screwdriver or remover, remove the rear seat back panel (A).
9. | Disconnect the protector (A).
10. | Remove the rear seat back panel (A) from the rear seat back frame (B).
11. | Pull out the headrest guides (A) while pinching the end of the guides, and remove them.
12. | Remove the rear seat back cover from the rear seat back frame.
13. | After removing the velcro tape (B) on the rear of seat back and remove the seat back cover (A).
14. | Installation is the reverse of removal.
• | Replace any damage clips.
Rear Seat Latch Replacement [LH]
• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts your hands.
• | Put on gloves to protect your hands.
1. | Remove the following items first.
A. | Rear seat assembly
B. | Rear seat back cover
2. | After loosening the mounting bolts, then remove the rear seat latch assembly (A).
3. | Installation is the reverse of removal.
• | Replace any damage clips.
Seat Back Cover Replacement [RH]
• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts your hands.
• | Put on gloves to protect your hands.
1. | Remove rear seat back assembly.
2. | Push the lock pin (B), remove the headrest (A).
3. | Remove the rear seat folding lever (A) after turning in the counter clock-wise direction.
4. | Remove the rear seat folding lever cover (B).
5. | After loosening the mounting screws, then remove the rear seat latch cover (A).
6. | Using a screwdriver or remover, remove the rear seat side bracket cover (A).
7. | Push the protecter (B) by the rear seat back panel (A).
8. | Using a screwdriver or remover, remove the rear seat back panel (A).
9. | Disconnect the protector (A).
10. | Remove the rear seat back panel (A) from the rear seat back frame (B).
11. | Pull out the headrest guides (A) while pinching the end of the guides, and remove them.
12. | Remove the rear seat back cover from the rear seat back frame.
13. | After removing the velcro tape (B) on the rear of seat back and remove the seat back cover (A).
14. | Installation is the reverse of removal.
• | Replace any damage clips.
Rear Seat Latch Replacement [RH]
• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts your hands.
• | Put on gloves to protect your hands.
1. | Remove the following items first.
A. | Rear seat assembly
B. | Rear seat back cover
2. | After loosening the mounting bolts, then remove the rear seat latch assembly (A).
3. | Installation is the reverse of removal.
• | Replace any damage clips.
Rear Seat Cushion Cover Replacement
• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts your hands.
• | Put on gloves to protect your hands.
1. | Remove the following items first.
A. | Rear seat cushion assembly
2. | After loosening the mounting screws, then remove the rear seat cup holder panel assembly (A).
3. | Remove the mounting clips (A).
4. | After removing the hog-ring clips (B) on the rear of seat cushion and remove the seat cushion cover (A).
5. | Installation is the reverse of removal.
• | To prevent wrinkles, make sure the material is stretched evenly over the cover (B) before securing the hog-ring clips (A).
• | Replace the hog-ring clips with new ones using special tool [C (09880-4F000)].