| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body (Interior and Exterior) > Bumper > Rear Bumper>Repair procedures |

Replacement
• | Put on gloves to protect your hands.
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Take care not bend or scratch the cover and other parts.
1. | After loosening the mounting screws, then remove the rear combination lamp (A).
2. | Push the lock pin, disconnect the connector (B).
3. | After loosening the rear bumper side’s mounting screw, then disconnect the side’s.
4. | Remove the rear bumper lower mounting clips.
5. | Loosen the mounting bolts.
6. | After loosening the mounting screw and clip, then remove the rear bumper (A).
7. | Push the lock pin, disconnect the rear bumper main connector (A).
8. | Installation is the reverse of removal.
• | Make sure the connector is plugged in properly.
• | Replace any damage clips.