| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Cylinder Block > Rear Oil Seal>Repair procedures |

Removal
1. | Remove the transaxle assembly. (Refer to transaxle - "Manual Transaxle assembly, Auto Transaxle assembly")
2. | MT : Remove the flywheel. (Refet to Cylinder Block - "Flywheel")
3. | AT : Remove the drive plate. (Refet to Cylinder Block - "Drive Plate")
4. | Remove the rear oil seal(A).
Installation
1. | Install the rear oil seal.
(1) | Apply engine oil to a new oil seal lip.
(2) | Using the SST(09231-H1100, 09231-2B200) and a hammer, tap in the oil seal until its surface is flush with the rear oil seal retainer edge.
2. | MT : Install the flywheel. (Refet to Cylinder Block - "FlyWheel")
3. | AT : Install the drive plate. (Refet to Cylinder Block - "Drive Plate")
4. | Install the transaxle assembly. (Refer to transaxle - "Manual Transaxle assembly, Auto Transaxle assembly")