| VELOSTER(FS) >2013 > G 1.6 T-GDI > Fuel System > Engine Control System > Waste Gate Solenoid Valve (WGV)>Repair procedures |

Inspection
1. | Turn the ignition switch OFF.
2. | Disconnect the WGV connector.
3. | Measure resistance between the WGV terminals 1 and 2 [B1/S1].
4. | Check that the resistance is within the specification.
Specification: Refer to "Specification"
Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Disconnect the waste gate solenoid valve connector (A).
3. | Disconnect the vapor hoses (B) from the waste gate solenoid valve.
4. | Remove the valve after removing the bolt (C).
5. | Remove the waste gate solenoid valve (D).
Installation
• | Install the component with the specified torques.
• | Note that internal damage may occur when the component is dropped. If the component has been dropped, inspect before installing.
1. | Installation is reverse of removal.