| VELOSTER(FS) >2013 > G 1.6 T-GDI > Restraint (Depowered) > SRSCM > Side Impact Sensor (SIS)>Repair procedures |

Removal
Side Impact Sensor
1. | Disconnect the battery negative cable and wait for at least three minutes before beginning work.
2. | Remove the door scuff trim. (Refer to the Body group - "Interior trim")
3. | Remove the center pillar lower trim. (Refer to the Body group - "Interior trim")
4. | Disconnect the side impact sensor connector (A).
5. | Loosen the side impact sensor mounting bolt (B) and remove the side impact sensor.
Installation
Side Impact Sensor
• | Do not turn the ignition switch ON and do not connect the battery cable while replacing the side impact sensor.
1. | Install the new side impact sensor with the bolt then connect the side impact sensor connector.
Tightening torque: 7.0 ~ 9.0 N.m (0.71 ~ 0.92 kgf.m, 5.2 ~ 6.6 lb-ft)
2. | Install the center pillar lower trim. (Refer to the Body group - "Interior trim")
3. | Install the door scuff trim. (Refer to the Body group - "Interior trim")
4. | Reconnect the battery negative cable.
5. | After installing the Side Impact Sensor, confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.