| VELOSTER(FS) >2013 > G 1.6 T-GDI > Clutch System > Clutch System > Clutch Master Cylinder>Repair procedures |

Removal
• | Do not spill brake fluid on the vehicle; it may damage the paint if brake fluid does contact the paint, wash it off immediately with water.
1. | Disconnect the push rod from the master cylinder by removing the snap pin (A) and washer (B).
2. | Remove the battery and ECM. (Refer to "Manual transaxle system" in MT group)
3. | Disconnect the clutch tube (B) and reservoir hose (A) from the clutch master cylinder.
4. | Remove the clutch master cylinder assembly (A) by turning it clockwise.
Installation
1. | Installation is in reverse order of removal.
• | GDI: Perform bleeding air procedure in clutch release cylinder after pouring the brake fluid. (Refer to Clutch Release Cylinder - "Adjustment")
• | T-GDI: Perform bleeding air procedure in concentric slave cylinder after pouring the brake fluid. (Refer to Concentric Slave Cylinder Assembly - "Adjustment")