| VELOSTER(FS) >2013 > G 1.6 T-GDI > Restraint (Depowered) > Airbag Module > Curtain Airbag (CAB) Module>Repair procedures |

Removal
1. | Disconnect the battery negative cable and wait for at least 3 minutes before beginning work.
2. | Remove the roof trim. (Refer to the Body group - "Interior")
3. | Disconnect the curtain airbag harness connector (A).
4. | After loosening the mounting bolts remove the curtain airbag.
Installation
1. | Remove the ignition key from the vehicle.
2. | Disconnect the battery negative cable and wait for at least three minutes.
3. | Tighten the curtain airbag mounting bolts.
Tightening torque: 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb.ft)
• | Never twist the airbag module when installing it. If the module is twisted, airbag module may operate abnormally.
4. | Connect the curtain airbag connector.
5. | Install the roof trim. (Refer to the Body group - "Interior")
6. | Reconnect the battery negative cable.
7. | After installing the curtain airbag (CAB), confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.