| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Smart key System > Smart key unit>Repair procedures |

Inspection
Smart Key Unit
- | Refer to the BE group - inspection / self diagnosis with GDS.
Smart Key Switch
- | Refer to the BE group - inspection / self diagnosis with GDS.
Antenna
- | Refer to the BE group - inspection / self diagnosis with GDS.
Tailgate Switch
1. | Check for continuity between the Trunk lid open switch terminals. [with Back View Camera] 1. Ground 2. Tailgate switch [without Back View Camera] 1. Ground (Tailgate) 2. Tailgate switch 3. Ground (Back View Camera) 4. Power 5. V-OUT 6. V-GND
2. | If continuity is not specified, inspect the switch
Removal
Smart key unit
1. | Disconnect the negative(-) battery terminal.
2. | Remove the AVN head unit. (Refer to the BE group - "AVN system - AVN Head Unit")
3. | Remove the smart key unit(A) with loosening bolt and nut, then disconnect the connector. [USA] [CANADA]
Interior #1 antenna
Take care not to scratch the crash pad and related parts.
1. | Disconnect the negative(-) battery terminal.
2. | Remove the console. (Refer to the BD group - "Console")
3. | Remove the multimedia jack.
4. | Disconnect the connector, then remove the interior #1 antenna(A) after loosening 2 screws.
Interior #2 antenna
Take care not to scratch the crash pad and related parts.
1. | Disconnect the negative(-) battery terminal.
2. | Remove the console. (Refer to the BD group - "Console")
3. | Disconnect the connector, then remove the interior #2 antenna(A) after loosening 2 screws.
Trunk antenna
1. | Disconnect the negative(-) battery terminal.
2. | Remove the trunk transverse trim. (Refer to the BD group - "Interior trim")
3. | Disconnect the connector, then remove the trunk antenna(A) after loosening 2 nuts.
Exterior Bumper Antenna
1. | Disconnect the negative(-) battery terminal.
2. | Remove the rear bumper. (Refer to the BD group - "Rear bumper")
3. | Disconnect the connector, then remove the rear bumper antenna(A) after loosening 2 screws.
Buzzer
1. | Disconnect the negative(-) battery terminal.
2. | Remove the air duct.
3. | Remove the buzzer(A) after disconnecting the connector.
Door outside handle
1. | Disconnect the negative(-) battery terminal.
2. | Remove the front door trim. (Refer to the BD group - "Front door")
3. | Remove the door outside handle connector. [Driver] [Assistant]
4. | Remove the outside handle cover(A) after loosening the mounting bolt.
Tailgate switch
1. | Disconnect the negative(-) battery terminal.
2. | Remove the tailgate outside handle(A) after loosening the mounting nut(3EA).
3. | Remove the tailgate switch assembly after loosening the screw(2EA).
4. | Remove the tailgate switch after loosening the screw(2EA).
Installation
Smart Key Unit
1. | Install the smart key unit.
2. | Connect the connector and install the smart key unit.
3. | Install the AVN head unit.
4. | Install the negative (-) battery terminal and check the smart key system.
Interior #1 Antenna
1. | Install the interior #1 antenna.
2. | Install the multimedia jack and the console.
3. | Install the negative (-) battery terminal and check the smart key system.
Interior #2 Antenna
1. | Install the interior #2 antenna.
2. | Install the console.
3. | Install the negative (-) battery terminal and check the smart key system.
Trunk Antenna
1. | Install the trunk antenna.
2. | Install the trunk transverse trim.
3. | Install the negative (-) battery terminal and check the smart key system.
Exterior Bumper Antenna
1. | Install the exterior bumper antenna.
2. | Install the rear bumper.
3. | Install the negative (-) battery terminal and check the smart key system.
Buzzer
1. | Install the buzzer.
2. | Install the air duct.
3. | Install the negative (-) battery terminal and check the smart key system.
Door Outside Handle
1. | Install the door outside handle.
2. | Install the door trim.
3. | Install the negative (-) battery terminal and check the smart key system.
Tailgate switch
1. | Install the tailgate switch.
2. | Install the tailgate outside handle.
3. | Install the negative (-) battery terminal and check the smart key system.