| VELOSTER(FS) >2013 > G 1.6 T-GDI > Restraint (Advanced) > Seat Belt Pretensioner > Anchor Pretensioner (APT)>Repair procedures |

Removal
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | Remove the seat belt after pushing the lock pin (A).
3. | Remove the following parts. (Refer to the Body group - "Interior trim")
A. | Door scuff trim
B. | Center pillar trim
4. | Disconnect the anchor pretensioner connector (A).
5. | Loosen the anchor pretensioner mounting bolt (B) and remove the anchor pretensioner.
Installation
1. | Remove ignition key from the vehicle.
2. | Disconnect the negative (-) cable from battery and wait for at least three minutes.
3. | Install the anchor pretensioner with mounting bolt.
Tightening torque : 39.2 ~ 53.9 N.m(4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
4. | Connect the anchor pretensioner connector.
5. | Install the following parts. (Refer to the Body group - "Interior trim")
A. | Center pillar trim
B. | Door scuff trim
6. | Insert the seat belt to the anchor pretensioner (A).
Make sure the lock pin is connected in properly.
7. | Reconnect the battery negative cable.
8. | After installing the anchor pretensioner, confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.