| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Button Engine Start System > Start/Stop Button>Repair procedures |

Removal
1. | Disconnect the negative(-) battery terminal.
2. | Remove the center fascia panel assembly (A).
3. | Disconnect the connector after loosening 2 screws, and then remove the start/stop button (A).
Installation
1. | Install the start/stop button.
2. | Install the center fascia panel assembly.