| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Intake And Exhaust System > Muffler>Repair procedures |

Removal and Installation
1. | Disconnect the battery negative terminal.
2. | Disconnect the rear oxygen sensor connector (A).
3. | Remove the rear oxygen sensor. (Refer to Fuel System - "Oxygen Sensor")
4. | Remove the front muffler (A).
Tightening torque: 39.2 ~ 58.8 N.m (4.0 ~ 6.0 kgf.m, 28.9 ~ 43.4 lb-ft)
5. | Remove the center muffler (A).
Tightening torque : 39.2 ~ 58.8N.m (4.0 ~ 6.0kgf.m, 28.9 ~ 43.4lb-ft)
6. | Remove the main muffler (A).
Tightening torque : 39.2 ~ 58.8N.m (4.0 ~ 6.0kgf.m, 28.9 ~ 43.4lb-ft)
7. | Install in the reverse order of removal.
When installing, replace with new gaskets.