| TIBURON(GK) >2004 > G 2.0 DOHC > Body Electrical System > Keyless Entry And>Components and Components Location |

BODY CONTROL MODULE (BCM)
BCM TERMINAL CONNECTION
Connector | Terminal No. | Description
A | 1 | NC
2 | NC
3 | Not used
4 | ESPS (IG1)
5 | SEAT BELT BUCKLE (RH)
6 | SEAT BELT BUCKLE (LH)
7 | CRASH SIGNAL
8 | NC
9 | A/BAG DIAG (FROM ESPS)
10 | A/BAG WARN'G IND
C | 1 | H/LAMP LOW RLY (S2)
2 | Not used
3 | FRONT WIPER RLY CONTROL
4 | FRONT FOG RLY-S2
5 | TURN SIGNAL (FR)
6 | Not used
7 | Not used
8 | FRONT WIPER RLY (IG2)
9 | TURN SIGNAL (FL)
10 | POSITION LAMP (RH)
11 | POSITION LAMP (LH)
12 | ABS MODULE (IG1)
13 | ALT 'L'
14 | FUSE & RLY BOX (IG2)
15 | WIPER PARK OUTPUT
16 | WASHER MOTOR
17 | NC
18 | NC
D | 1 | B+ 50A
E | 1 | NC
2 | TAILGATE LOCK SW
3 | ASSIST DOOR LOCK SW
4 | ASSIST DOOR SW
5 | Not used
6 | TAILGATE SW
7 | NC
8 | DRIVER DOOR LOCK SW
9 | DRIVER DOOR SW
10 | SEAT BELT SW
11 | NC
12 | NC
F | 1 | Not used
2 | BACKUP LAMP
3 | Not used
4 | OUTSIDE MIRROR
5 | TAIL LAMP (RH)
6 | DOOR LOCK FEED
7 | NC
8 | DOOR UNLOCK FEED
9 | NC
10 | TAIL LAMP (LH)
11 | 4 DOOR SW
12 | Not used
13 | TURN SIGNAL (RL)
14 | NC
15 | LUGGAGE LAMP
16 | NC
17 | TURN SIGNAL (RR)
18 | AMP
19 | OUTSIDE MIRROR HEATER
20 | Not used
21 | REAR WIPER MOTOR (IG2)
22 | TAILGATE OPEN SW
G | 1 | REAR HEATED
2 | POWER WINDOW SW
H | 1 | IMMOBILIZER ANTENNA 1
2 | NC
3 | TURN SIGNAL SW (RH)
4 | DOOR WARN'G SW
5 | TAIL SW
6 | Not used
7 | CODE SAVER
8 | NC
9 | HOOD SW
10 | NC
11 | IMMOBILIZER ANTENNA 2
12 | EXPORT GND INPUT
13 | TURN SIGNAL SW (LH)
14 | AUTO LIGHT SW INPUT
15 | NC
16 | HEAD LAMP SW
17 | FRONT FOG SW
18 | HAZARD SW
19 | REAR DEFOG SW
20 | Not used
I | 1 | AIR CONDITIONER SW
2 | CLUSTER BATTERY CHARGE
3 | Not used
4 | TCS SW (IG1)
5 | CLUSTER (IG1)
6 | CLUSTER (IG1)
7 | CLUSTER (T/SIG LH OUT)
8 | ECU (IG1)
9 | CLUSTER (T/SIG RH OUT)
10 | RR HTD SW (FOR INDICATOR)
11 | CLUSTER (A/BAG IND)-IG1
12 | HI-SCAN (B+)
13 | DIGITAL CLOCK (ACC)
14 | IMMOBILIZER INDICATOR
15 | EXTERNAL TAIL LAMP (RH)
16 | HI-SCAN (A/BAG DIAGNOSIS)
17 | AIR CONDITIONER (IG2)
18 | AUTO LIGHT GND
19 | DIAGNOSIS & CODE SAVING
20 | IMMOBILIZER W LINE
J | 1 | MULTI-FUNCTION INT(T) GND
2 | SIREN CONTROL
3 | KEY HOLE ILL.
4 | SPEED SENSOR
5 | INTERIOR ILL.
6 | CLUSTER (A/BAG WARN'G IND)
7 | DCT
8 | DOOR AJAR
9 | MULTI-FUNCTION INT
10 | MULTI-FUNCTION INT (T)
11 | AUTO LIGHT SIGNAL
12 | Not used
13 | OVER SPEED GND (CLUSTER)
14 | NC
15 | AUTO LIGHT SUPPLY
16 | TAILGATE OPEN IND
K | 1 | CIGAR LIGHTER
2 | WIPER LOW
3 | WIPER HI
4 | BACKUP SW
5 | AUDIO (ACC)
6 | MULTI-FUNCTION WASHER SW
7 | BACKUP LAMP SW
8 | START INHIBIT RELAY
9 | SEAT HEATER SW (IG2)
10 | JOINT MAIN 3 (B+)
11 | STOP SW (B+)
12 | IGNITION COIL (V6)
13 | Not used
14 | WIPER PARK'G
L | 1 | GND 1
2 | NC
3 | BLOWER MOTOR
4 | IG SW (IG1)
5 | GND 2
6 | WIPER SW POWER
7 | IG SW (ACC)
8 | IG SW (IG2)
M | 1 | SUNROOF (IG2)
2 | ROOM LAMP (B+)
3 | ROOF LAMP DECAY CONTROL
4 | ECM
5 | Not used
6 | S/ROOF & ROOM LAMP GND
7 | ECM MIRROR
8 | SUNROOF MOTOR (B+)
FUSE
Fuse No. | Capacity | Connection circuit
1 | 20A | Ignition coil (2.7L), Electronic chrome mirror
2 | 20A | AMP
3 | 10A | Back-up lamp switch, Transaxle range switch, Cruise control module, Stop lamp switch
4 | 10A | Instrument cluster (A/BAG IND.)
5 | 15A | Air bag control module, Seat belt buckle switch
6 | 10A | Mirror defogger
7 | 10A | Hazard relay
8 | 15A | Rear wiper motor, Rear wiper relay
9 | 10A | Right tail lamps, Glove box lamp
10 | 20A | Front wiper motor, Front wiper relay
11 | 10A | Blower relay, Blower motor
12 | 30A | Defogger relay
13 | 15A | Stop lamp switch, Burglar alarm horn relay
14 | 10A | Left tail lamps
15 | 10A | A/C control module, Blower relay
16 | 10A | ECM, Multi gauge unit, TCM, Vehicle speed sensor
17 | 10A | Instrument cluster (Power), Pre-excitation resistor, DRL control module, Generator
18 | 10A | Room lamp, Clock, Audio, Data link connector, Multi gauge unit
19 | 30A | Power window relay
20 | 15A | Trunk lid switch
21 | 10A | A/C relay, AQS sensor, Head lamp relay, DRL control module
22 | 10A | Not used
23 | 15A | Cigarette lighter, Outside mirror switch
24 | 15A | Sunroof, Power door lock/unlock relay
25 | 20A | Seat warmer
26 | 10A | ABS control module, TCS switch
27 | 10A | Audio, Digital clock
- | 10/15A 20/30A | Spare fuse