| TIBURON(GK) >2004 > G 2.7 DOHC > Steering System > General Information>Special Service Tools |

SPECIAL TOOLS
Tool (Number and name) | Illustration | Use
09222-32100 Valve stem oil seal installer |  |
1. | Installation of the ball bearing to rack housing
2. | Installation of the oil seal to oil pump
09432-21600 Bearing installer |  |
1. | Installation of the needle bearing to rack housing
2. | Installation of the ball bearing and oil seal to valve body
09434-14200 Counter shaft bearing installer |  | Installation of the oil seal to rack bushing and valve body
09555-21000 Bar |  | Removal and installation the oil seal.
09561-11002 Steering wheel puller |  | Removal of the steering wheel.
09565-11100 Preload socket |  | Measurement of the mainshaft preload.
09568-31000 Tie rod end puller |  | Seperation of the tie rod end ball joint.
09572-21000 Oil pressure gauge |  | Measurement of the power steering oil pressure. (use with 09572-22100, 09572-21200)
09572-21200 Oil pressure gauge adapter (Hose side) |  | Measurement of the power steering oil pressure. (use with 09572-21000, 09572-22100)
09572-22100 Oil pressure gauge adapter (Pump side) |  | Measurement of the power steering oil pressure. (use with 09572-21000, 09572-21200)
09573-21000 Oil seal installer guide |  | Installation of the oil seal (use with 09573-21100, 09573-21200, 09517-11000, 09555-21000)
09573-21100 Oil seal installer |  | Installation of the oil seal (use with 09573-21000, 09573-21200, 09555-21000)
09573-21200 Oil seal guide |  | Removal and installation of the oil seal