| TIBURON(GK) >2006 > G 2.0 DOHC > Brake System > General Information>Troubleshooting |

TROUBLESHOOTING
PROBLEM SYMPTOMS TABLE
Symptom | Suspect Area | Remedy
Lower pedal or spongy pedal |
1. | Brake system (Fluid leaks)
2. | Brake system (Air in)
3. | Piston seals (Worn or damaged)
4. | Master cylinder (Faulty)
| Correct Bleeding Replace Replace
Brake drag |
1. | Brake pedal freeplay (Minimal)
2. | Parking brake lever travel (Out of adjustment)
3. | Parking brake wire (Sticking)
4. | Pad (Cracked or distorted)
5. | Piston (Stuck)
6. | Piston (Frozen)
7. | Booster system (Vacuum leaks)
8. | Master cylinder (Faulty)
| Adjust Adjust Correct Replace Replace Replace Replace Replace
Brake pull |
1. | Pad (Oily)
2. | Piston (Frozen)
3. | Disc (Scored)
4. | Pad (Cracked or distorted)
| Replace Replace Replace Replace
Hard pedal but brake inefficient |
1. | Brake system (Fluid leaks)
2. | Brake system (Air in)
3. | Pad (Worn)
4. | Pad (Cracked or distorted)
5. | Pad (Oily)
6. | Pad (Glazed)
7. | Disc (Scored)
8. | Booster system (Vacuum leaks)
| Correct Bleeding Replace Replace Replace Replace Replace Replace
Noise from brake |
1. | Pad (Cracked or distorted)
2. | Installation bolt (Loosen)
3. | Disc (Scored)
4. | Pad retainers (Loosen)
5. | Sliding pin (Worn)
6. | Pad (Dirty)
7. | Pad (Glazed)
8. | Brake pad shim (Damage)
| Replace Retighten Replace Replace Replace Clearing Replace Replace