| TIBURON(GK) >2007 > G 2.0 DOHC > Body Electrical System > Immobilizer System>Troubleshooting |

DIAGNOSIS OF IMMOBILIZER FAULTS
• | Communication between the ECM and the BCM
• | Function of the BCM and the transponder, and
• | Data (stored in the ECM) related to the immobilizer function.
Type | Diasnostic Codes | Immobilizer Related Faults
SMARTRA (2.0β ENGINE) | P1690 | SMARTRA ERROR
P1691 | ANTENNA ERROR
P1693 | TRANSPONDER ERROR
P1694 | ECU SIGNAL ERROR
P1695 | EEPROM ERROR
P1696 | MISMATCH/OVERTRIAL ERROR
STAND ALONE (2.7δ ENGINE) | 01 | Untaught transponder
02 | Transponder communication error
03 | ECM communication error
04 | Immobilizer antenna error - open
05 | BCM internal fault or EEPROM
06 | ECM not detected
P1642 | Non-Immobilizer-EMS connected to an Immobilizer
REPLACEMENT OF ECM AND BCM NEUTRALISING ECM