| TIBURON(GK) >2007 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Air conditioning System > Condenser fan & relay>Repair procedures |

CHECKING
CONDENSER
1. | Check condenser pin for clogging and damage. If clogged, clean it with water, and blow it with compressed air. If bent, gently stretch it using a screwdriver or pliers.
2. | Check the condenser connection area for leakage, and repair or replace if required.
CONDENSER FAN
1. | Check the connector for connection condition.
2. | Check the condenser fan motor using battery voltage.