| TIBURON(GK) >2007 > G 2.0 DOHC > Driveshaft and axle > General Information>Troubleshooting |

TROUBLESHOOTING
Symptom | Possible cause | Remedy
Vehicle pulls to one side | Galling of drive shaft ball joint Wear, rattle or galling of wheel bearing Defective front suspension and steering | Replace Replace Adjust or replace
Vibration | Wear, damage or bending of drive shaft Drive shaft rattle and hub serration Wear, rattle or scratching of wheel bearing | Replace Replace Replace
Shimmy | Improper wheel balance Defective front suspension and steering | Adjust or replace Adjust or replace
Excesive noise | Wear, damage or bent drive shaft Drive shaft rattle and hub serration Drive shaft rattle and side gear serration Wear, rattle or galling of wheel bearing Loose hub nut Defective front suspension and steering | Replace Replace Replace Replace Adjust or replace Adjust or replace