| TIBURON(GK) >2007 > G 2.0 DOHC > Restraint > Seat Belt Pretensioner > Seat Belt Retractor Pretensioner (BPT)>Description and Operation |

DESCRIPTION
Never attempt to measure the circuit resistance of the Seat Belt Pretensioner (BPT) even if you are using the specified tester. If the circuit resistance is measured with a tester, the pretensioner will be ignited accidentally. This will result in serious personal injury.