| TIBURON(GK) >2007 > G 2.7 DOHC > Heating,Ventilation, Air Conditioning > Air conditioning System > Water temperature sensor>Description and Operation |

DESCRIPTION
1. | Water temperature sensor is located at the heater unit.
2. | It detects coolant temperature. Its signal is used for cold engine lockout control. When the driver operates the heater before the engine is warmed up, the signal from sensor causes the heater control unit to reduce blower motor speed until coolant temperature reaches the threshold value.