| TIBURON(GK) >2008 > G 2.0 DOHC > Body Electrical System > Keyless Entry And Burglar Alarm>Components and Components Location |

BODY CONTROL MODULE (BCM)
BCM TERMINAL CONNECTION
Connector | Pin | Description
BCM-AI | 1 | -
2 | -
3 | -
4 | ESPS (IG1)
5 | RH seat belt buckle
6 | LH seat belt buckle
7 | Crash signal
8 | -
9 | Airbag diagnosis ( From ESPS)
10 | Airbag warning lamp
BCM-CE | 1 | Head lamp low relay (S2)
2 | DRL unit NO 12
3 | Front wiper relay control
4 | Front fog relay (S1)
5 | Turn signal lamp (FR)
6 | Tail auto cut to DRL
7 | DRL unit (11)
8 | Front wiper relay (IG2)
9 | Turn signal lamp (FL)
10 | Position lamp (RH)
11 | Position lamp (LH)
12 | ABS module (IG1)
13 | ALT 'L'
14 | Fuse & relay box (IG2)
15 | Wiper park output
16 | Washer motor
17 | -
18 | -
BCM-DE | 1 | B+50A
BCM-EF | 1 | Assist door key switch
2 | Tail gate lock switch
3 | Assist door lock switch
4 | Assist door switch
5 | Folding switch
6 | Tail gate open switch
7 | Driver door key unlock switch
8 | Driver door lock switch
9 | Driver door switch
10 | Seat belt switch
11 | -
12 | -
BCM-FF | 1 | Rear fog lamp relay
2 | Back up lamp
3 | -
4 | Outside mirror
5 | Tail lamp (RH)
6 | Door lock feed
7 | -
8 | Door unlock feed
9 | -
10 | Tail lamp (LH)
11 | 4 Door switch
12 | Mirror unfolding/Ass door unlock feed
13 | Turn signal (RL)
14 | -
15 | Luggage lamp
16 | -
17 | Turn signal (RR)
18 | AMP
19 | Outside mirror heater
20 | Mirror folding
21 | Rear wiper motor (IG2)
22 | Tail gate open switch
BCM-GF | 1 | Rear window defogger
2 | Power window switch
BCM-HM | 1 | Immobilizer antenna 1
2 | 2 Stage unlock GND
3 | Turn signal switch (RH)
4 | Door warning switch
5 | Tail lamp switch
6 | Rear fog lamp switch
7 | Code saver
8 | -
9 | Hood switch
10 | -
11 | Immobilizer antenna 2
12 | Export ground
13 | Turn signal lamp switch
14 | Auto light switch input
15 | -
16 | Head lamp switch
17 | Front fog lamp switch
18 | Hazard lamp switch
19 | Rear defogger switch
20 | Rear fog lamp indicator
BCM-IM | 1 | Air conditioner switch
2 | Cluster battery charge
3 | -
4 | ESP switch (IG1)
5 | Cluster (IG1)
6 | Cluster (IG2)
7 | Cluster (Turn sig LH out)
8 | ECU (IG1)
9 | Cluster (Turn sig RH out)
10 | RR HTD switch
11 | Cluster (Airbag indicator)
12 | Diagnostic tool (B+)
13 | Digital clock (ACC)
14 | Immobilizer indicator
15 | External tail lamp (RH)
16 | Diagnostic tool (A/bag)
17 | Air conditioner (IG2)
18 | Auto light ground
19 | Diagnosis & code saving
20 | Immobilizer
BCM-JM | 1 | Multifunction switch- Intermittent wiper ground
2 | Siren control
3 | Key hole illumination
4 | Speed sensor
5 | Interior illumination
6 | Cluster (A/BAG warning indicator)
7 | DCT
8 | Door open indicator
9 | Multifunction INT
10 | Multifunction INT (T)
11 | Auto light signal
12 | Seat belt indicator
13 | Over speed ground
14 | -
15 | Auto light supply
16 | Tail gate open indicator
BCM-KM | 1 | Cigar lighter
2 | Wiper low
3 | Wiper high
4 | Back up switch
5 | ACC
6 | Washer switch
7 | Back up lamp switch
8 | Start inhibit relay
9 | Seat heater switch (IG2)
10 | Joint main 3 (B+)
11 | Stop switch (B+)
12 | Ignition coil
13 | -
14 | Wiper parking
BCM-LM | 1 | Ground 1
2 | -
3 | Blower motor
4 | Ignition switch (IG1)
5 | Ground 2
6 | Wiper switch power
7 | Ignition switch (ACC)
8 | Ignition switch (IG2)
BCM-MR | 1 | Sunroof (IG2)
2 | Roof lamp (B+)
3 | Roof lamp decay control
4 | ECM
5 | -
6 | Sunroof & room lamp GND
7 | ECM mirror
8 | Sunroof (B+)
FUSE
NO. | CAPACITY | DESCRIPTION
1 | 20A | Ignition coil (2.7L), Electronic chrome mirror
2 | 20A | AMP
3 | 10A | Back-up lamp switch, Transaxle range switch, Stop lamp switch
4 | 10A | Instrument cluster (Airbag indicator)
5 | 15A | Airbag control module , Seat belt buckle switch
6 | 10A | Mirror defogger
7 | 10A | Hazard lamp relay
8 | 15A | Rear wiper motor, Rear intermittent wiper relay
9 | 10A | Right tail lamps, Glove box lamp
10 | 20A | Front wiper motor, Front wiper relay
11 | 10A | Blower relay, Blower motor
12 | 30A | Defogger relay
13 | 15A | Stop lamp switch, Folding /unfolding relay, Burglar alarm horn relay
14 | 10A | Left tail lamps
15 | 10A | A/C control module, Blower relay
16 | 10A | ECM, Multi gauge unit, TCM, Vehicle speed sensor
17 | 10A | Instrument cluster(Power), Alternator resister, DRL Control module, Pre-excitation resistor
18 | 10A | Room lamp, Clock, Audio, Data link connector, Multi gauge unit
19 | 30A | Power window relay
20 | 15A | Trunk lid switch
21 | 10A | AQS sensor, Head lamp relay, DRL Control module
22 | - | -
23 | 15A | Cigar lighter, Outside mirror switch
24 | 15A | Sunroof , Power door lock/unlock relay
25 | 20A | Seat heater
26 | 10A | ESP/ABS control module
27 | 10A | Audio, Clock