| TIBURON(GK) >2008 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Blower > Control Panel>Schematic Diagrams |

CONNECTOR CONFIGURATIONS
Connector | Pin No. | Name | Connector | Pin No. | Name
Blower switch | 1 | MIDDLE HIGH | Main switch | 11 | SENSOR GROUND
2 | COMMON | 12 | FRE.
3 | GROUND | 13 | REC.
4 | HIGH | 14 | ILL+
5 | MIDDLE LOW | 15 | ILL-
6 | LOW | 16 | COMMON (BLOWER)
Main switch | 1 | IGN2 | 17 | A/C OUTPUT
2 | B+ | 18 | HUMIDITY (Rear defogger)
3 | GROUND | 19 | S/W (Rear defogger)
4 | MODE ACT. (VENT) | 20 | -
5 | MODE ACT. (DEF) | 21 | -
6 | MODE F/B | 22 | -
7 | TEMP ACT. (WARM) | 23 | -
8 | TEMP ACT. (COOL) |  |
9 | TEMP F/B |  |
10 | VCC |  |
SCHEMATIC DIAGRAM
BLOWER S/W
WIRING DIAGRAM