| TIBURON(GK) >2008 > G 2.7 DOHC > Emission Control System > General Information>Specifications |

SPECIFICATIONS
▷ Type : Piezo - Resistivity type ▷ Specification
Pressure (kPa) | Output Voltage (V)
-6.67 | 0.5
0 | 2.5
+6.67 | 4.5
▷ Specification
Item | Specification
Coil Resistance (Ω) | 24.5 ~ 27.5 Ω [20°C (68°F)]
▷ Specification
Item | Specification
Coil Resistance (Ω) | 23.9 ~ 26.9 Ω [20°C (68°F)]
TIGHTENING TORQUE
Item | N•m | kgf•m | lbf•ft
Positive Crankcase Ventilation Valve | 8.0 ~ 12.0 | 0.8 ~ 1.2 | 6.0 ~ 8.0