| TUCSON(LM) >2010 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Air Conditioning System > In car sensor>Description and Operation |

Description
1. | In-car air temperature sensor is located at the center facia lower panel.
2. | The sensor contains a thermistor which measures the temperature of the inside. The signal decided by the resistance value which changes in accordance with perceived inside temperature, is delivered to heater control unit and according to this signal the control unit regulates incar temperature to intended value.