| TUCSON(LM) >2010 > G 2.4 DOHC > Body Electrical System > Audio>Specifications |

Specifications
Audio
Item | Specification
Model | RADIO/CD/MP3 (PA710)
SDARS (Option) | ○ (PA710S)
Power supply | DC 14.4V
Rated output | Max 3.2Vrms
Antenna | 80PF 75Ω
Tuning type | PLL SYNTHESIZED TUNING
Frequency range / Channel space | FM | 87.5~107.9 MHz / 200KHz
AM | 530~1710 KHz (10KHz)
Speaker
Item | PA710/710S | AVN
Input Power (W or V) | Front | Max 40W
Rear | Max 40W
Front Tweeter | Max 40W
Sub woofer | - | MAX 40W
Speaker Impedance (Ω) | Front | 4 ± 0.6 | 2 ± 0.3
Rear | 4 ± 0.6 | 2 ± 0.3
Front Tweeter | 3.4 ± 0.5
Sub woofer | - | 2 ± 0.3
Speaker Number | 6 | 8