| TUCSON(LM) >2011 > G 2.0 DOHC > Body (Interior and Exterior) > General Information>Specifications |

Specifications
Items | Specification
Hood | Type | Rear hinged, front opening type
Front Door | Construction | Front hinged, full door construction
Regulator system | Wire-drum type
Locking system | Pin-fork system
Rear Door | Construction | Front hinged, full door construction
Regulator system | Wire-drum type
Locking system | Pin-fork system
Tail Gate | Type | Front hinged, gas lifter type
Seat Belts | Front | 3 point type with Emergency Locking Retractor (E.L.R)
Rear | 3 point type with Emergency Locking Retractor (E.L.R) 2 point type
Tightening Torque
Items | N.m | Kgf.m | lb-ft
Front andrear doors | Door hinge to body | 34.3 ~ 41.2 | 3.5 ~ 4.2 | 25.3 ~ 30.4
Door hinge to door | 9.8 ~ 19.6 | 1.0 ~ 2.0 | 7.2 ~ 14.5
Door checker to door | 3.9 ~ 5.9 | 0.4 ~ 0.6 | 2.9 ~ 4.3
Door checker to body | 16.7 ~ 21.6 | 1.7 ~ 2.2 | 12.3 ~ 15.9
Door glass mounting bolt | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Outside handle base mounting bolt | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Door channel mounting nuts | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Latch mounting bolts | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Door module mounting bolts | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Door striker mounting bolts | 8.8 ~ 13.7 | 0.9 ~ 1.4 | 6.5 ~ 10.1
Tail gate | Tail gate hinge to tail gate | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Tail gate hinge to body | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Tail gate latch mounting bolts | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Tail gate striker mounting bolts | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Hood | Hood hinge to body | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Hood hinge to hood | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Hood latch to body | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~ 8.7
Seat | Front seat mounting bolts | 44.1 ~ 58.8 | 4.5 ~ 6.0 | 32.5 ~ 43.4
Front seat frame mounting bolts | 44.1 ~ 58.8 | 4.5 ~ 6.0 | 32.5 ~ 43.4
Rear seat mounting bolts | 44.1 ~ 58.8 | 4.5 ~ 6.0 | 32.5 ~ 43.4
Seat belt | Height adjuster mounting bolts | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Front seat belt upper anchor mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Front seat belt lower anchor mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Front seat belt retractor mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Rear seat belt lower anchor mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Rear seat belt retractor mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Seat belt buckle mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Quarter fixed glass | Quarter fixed glass mounting nuts | 3.9 ~ 4.4 | 0.4 ~ 0.45 | 2.9 ~ 3.3
Outside rearview mirror | Outside rearview mirror mounting nuts | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Panoramaroof | Panoramaroof mounting nuts | 19.6 ~ 29.4 | 2.0 ~ 3.0 | 14.5 ~ 21.7
Panoramaroof mounting bolts | 19.6 ~ 29.4 | 2.0 ~ 3.0 | 14.5 ~ 21.7
Panoramaroof earthing mounting bolt | 10.8 ~ 13.7 | 1.1 ~ 1.4 | 8.0 ~ 10.1