| TUCSON(LM) >2011 > G 2.0 DOHC > Driveshaft and axle > General Information>Specifications |

Specification
Items | Inner side | Outer side
Front driveshaft | Joint type | VTJ | BJ
Max. permissible angle | 23.0° | 46.5°
Rear driveshaft | Joint type | TJ | BJ
Max. permissible angle | 23.0° | 46.5°
Rear differential | Oil type | Hypoid gear oil (API GL-5, SAE 75W/90)
Oil capacity (L) | About 0.6~0.7
Reduction gear type | Hypoid gear
Reduction gear ratio | 3.091
Final drive gear backlash mm(in.) | 0.1 ~ 0.15
Differential gear backlash mm(in.) | 0 ~ 0.05
Tightening torque
Items | Nm | Kgf.m | lb-ft
Front | Wheel nut | 88.3~107.9 | 9~11 | 65.1~79.6
Driveshaft nut | 196.1 ~ 274.5 | 20.0~28.0 | 144.6 ~ 202.5
Strut assembly lower mounting bolt | 137.2 ~ 156.9 | 14.0~16.0 | 101.2 ~ 115.7
Break caliper mounting bolt | 78.4 ~ 98.0 | 8.0~10.0 | 57.8 ~ 72.3
Wheel speed sensor mounting bolt | 6.9~10.8 | 0.7~1.1 | 5.1~8.0
Break disc mounting screw | 4.9~5.9 | 0.5~0.6 | 3.6~4.3
Lower arm assembly mounting bolt | 137.2~156.9 | 14~16 | 101.2~115.7
Lower arm ball joint mounting bolt | 98.1~117.7 | 10.0~12.0 | 72.3~86.8
Tie rod end ball joint mounting nut | 34.3 ~ 44.1 | 3.5~4.5 | 25.3 ~ 32.5
Rear | Wheel nut | 88.3~107.9 | 9.0~11.0 | 65.1~79.6
Driveshaft castle nut | 196.1 ~ 274.5 | 20.0~28.0 | 144.6 ~ 202.5
Shock absorber upper mounting nut | 137.2 ~ 156.9 | 14.0~16.0 | 101.2 ~ 115.7
Break caliper mounting bolt | 78.4 ~ 98.3 | 8.0~10.0 | 57.8 ~ 72.3
Wheel speed sensor mounting bolt | 6.9~10.8 | 0.7~1.1 | 5.1~8.0
Break disc mounting screw | 4.9~5.9 | 0.5~0.6 | 3.6~4.3
Hub assembly mounting bolt | 78.5~88.3 | 8.0~9.0 | 57.9~65.1
Upper arm ball joint mounting nut | 98.1 ~ 117.7 | 10.0~12.0 | 72.3 ~ 86.8
Lower arm mounting bolt | 137.3~156.9 | 14.0~16.0 | 101.3~115.7
Assist arm ball joint mounting nut | 137.2 ~ 156.9 | 14.0~16.0 | 101.2 ~ 115.7
Trailing arm mounting bolt | 34.3 ~ 53.9 | 3.5~5.5 | 25.3 ~ 39.7
Front propellershaft | Front propeller shaft mounting bolt | 49.0~68.6 | 5.0~7.0 | 36.2~50.6
Propeller shaft center bearing bracket mounting bolt | 49.0~53.9 | 5.0~7.0 | 36.2~50.6
Rear Differential | Rear propeller shaft mounting bolt | 49.0~68.6 | 5.0~7.0 | 36.2~50.6
Rear differential mounting bolt | 68.6~88.3 | 7.0~9.0 | 50.6~65.1
Differential cover mounting bolt | 39.2~49.0 | 4.0~5.0 | 28.9~36.2
Rear differential drain plug | 49.0~68.6 | 5.0~7.0 | 36.2~50.6
Rear differential filler plug | 39.2~58.8 | 4.0~6.0 | 28.9~43.3
Replace self-locking nuts with new ones after removal.
Lubricants
Items | Lubricants | Quantity
Front driveshaft | BJ | RBA | 100g
VTJ | CW-13TJ | 150g
Rear driveshaft | BJ | RBA | 60g
TJ | CW-13TJ | 90g