| TUCSON(LM) >2011 > G 2.4 DOHC > Clutch System > Clutch System > Clutch Pedal>Repair procedures |

Replacement
1. | Remove the flexible hose (A) connected to brake reserve tank from the master cylinder.
2. | Disconnect the clutch tube (B) from the master cylinder.
3. | Disconnect the two ignition lock switch connectors (C).
4. | Remove the clutch pedal mounting bolts (A-3ea) and the bracket mounting nuts (B-1ea.)
Tightening torque : 16.7~25.5N.m (1.7~2.6kgf.m, 12.3~18.8lb-ft)
5. | Installation is resverse of removal.