| TUCSON(LM) >2011 > G 2.4 DOHC > Clutch System > General Information>Specifications |

Specification
Item | Specification
Engine type | 2.4L
Clutch operation | Hydraulic type
Clutch disc | Single dry with diaphragm
Clutch cover assembly | Diaphram spring strap
Tightening Torque
Item | N.m | kgf.m | lb-ft
Clutch cover (2.4L) | 247.5~34.3 | 2.5~3.6 | 18~26
Concentric slave cylinder | 11.8~14.7 | 1.2~1.5 | 8.7~10.8
Stop lamp switch | 7.8~9.8 | 0.8~1.0 | 5.8~7.2
Ignition lock switch | 7.8~9.8 | 0.8~1.0 | 5.8~7.2
Air bleeding plug | 6.8~9.8 | 0.7~1.0 | 9.2~13.3
Clutch pedal mounting | 16.7~25.5 | 1.7~2.6 | 12.3~18.8
Lubricants
Item | Specified lubricants | Quantity
Inner surface of clutch disc spline | CASMOLY L9508 | 0.2 gr.
Clutch master cylinder tube | RG 306 | As required
Service Standard
Item | Standard value
Clutch pedal stroke | 147~153 mm (5.7874~6.0236 in.)
Clutch pedal free play | 6~13 mm (0.2362~0.5118 in.)
Distance between a mat and a clutch pedal | 167 mm (6.5748 in.)
Depth from a clutch lining surface to a rivet | 0.5 mm (0.1969 in.)