| TUCSON(LM) >2012 > G 2.4 DOHC > Automatic Transaxle System > General Information>Special Service Tools |

Special Service Tools
Tools (Number and name) | Illustration | Use
09200-38001 Engine support fixture (Beam) |  | Removal and installation of the transaxle. Except lower supporter, use beam only with new engine support fixture supporter(SST No.:09200-2S000)
09200-2S000 Engine support fixture (Supporter) |  | Removal and installation of the transaxle. Use this supporter with the upper beam of the engine support fixture(SST No.:09200-38001)
09453-3L241 Oil seal installer |  | Installation of transaxle case oil seal. [Using with handle (SST No.:09231-H1100)]
09231-H1100 Bar |  | Installation of transaxle case oil seal. [Using with oil seal installer (SST No.:09453-3L241)]