| TUCSON(LM) >2013 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Controller > Heater & A/C Control Unit(Manual)>Components and Components Location |

Components
Connector Pin Function
Connector | Pin No | Function | Connector | Pin NO | Function
Connector(A) | 1 | Middle High | Connector(B) | 1 | Tail Lamp (ILL+)
2 | - | 2 | Battery
3 | GND | 3 | Mode Actuator (VENT)
4 | High | 4 | Mode Actuator (DEF)
5 | Middle Low | 5 | Temp Actuator (COOL)
6 | Low | 6 | Temp Actuator (WARM)
| 7 | Intake Actuator (FRE)
8 | Intake Actuator (REC)
9 | -
10 | -
11 | Mode Actuator (F/B)
12 | Temp Actuator (F/B)
13 | Intake Actuator (F/B)
14 | Blower Motor Common (-)
15 | Blower F/B
16 | Rheostat (ILL-)
17 | IG2
18 | -
19 | Can (HIGH)
20 | Can (LOW)
21 | -
22 | ECV IN
23 | ECV OUT
24 | -
25 | Vref (+5V)
26 | Evaporator Sensor
27 | Ambient Sensor
28 | -
29 | -
30 | -
31 | Sensor GND
32 | GND