| TUCSON(LM) >2013 > G 2.0 DOHC > Body Electrical System > Lighting System > Luggage Room Lamp>Repair procedures |

Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the luggage room lamp (B) when prying the hole (A) with a flat-up screwdriver
3. | Remove the luggage room lamp bulb in case of necessity
Installation
1. | Replace the lamp bulb.
2. | Install the luggage room lamp assembly after connecting the lamp connector.