| TUCSON(LM) >2013 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Controller > Heater & A/C Control Unit(Dual)>Components and Components Location |

Components
Control Panel
Connector Pin Function
Connector | Pin NO | Function | Connector | Pin NO | Function
Connector(A) | 1 | Battery | Connector(B) | 1 | CAN (LOW)
2 | Tail Lamp (ILL+) | 2 | CAN (HIGH)
3 | IG2 | 3 | Intake Actuator (F/B)
4 | DR Temp Actuator (COOL) | 4 | Mode Actuator (F/B)
5 | DR Temp Actuator (WARM) | 5 | PS Temp Actuator (F/B)
6 | - | 6 | DR Temp Actuator (F/B)
7 | Mode Actuator (VENT) | 7 | Diagnosis (Cluster Ion)
8 | Mode Actuator (DEF) | 8 | ECV IN
9 | - | 9 | GND
10 | - | 10 | Hi-Scan (K-Line)
11 | - | 11 | Evaporator Sensor
12 | Rheostat (ILL-) | 12 | Ambient Sensor
13 | GND | 13 | Incar Sensor
14 | Vref +5V | 14 | DR Sun (-)
15 | Ion Signal | 15 | PS Sun (-)
16 | Intake Actuator (FRE) | 16 | ECV OUT
17 | Intake Actuator (REC) |  |
18 | Clean Signal |  |
19 | Blower Motor (+) |  |
20 | PS Temp Actuator (COOL) |  |
21 | PS Temp Actuator (WARM) |  |
22 | Power Mosfet (GATE) |  |
23 | Power Mosfet (DRAIN) |  |
24 | - |  |
25 | - |  |
26 | Sensor GND |  |