| TUCSON(LM) >2013 > G 2.4 DOHC > Manual Transaxle System > General Information>Troubleshooting |

Troubleshooting
Symptom | Probable cause | Remedy
Vibration, noise | Loose or damaged transaxle and engine mounts | Tighten or replace mounts
Inadequate shaft end play | Correct end play
Worn or damaged gears | Replace gears
Inadequate grade of oil | Replace with specified oil
Low oil level | Replenish
Inadequate engine idle speed | Adjust idle speed
Oil leakage | Broken or damaged, oil seal or O-ring | Replace control cable oil seal or O-ring
Hard shift | Faulty control cable | Replace control cable
Poor contact or wear of synchronizer ring and gear cone | Correct or replace
Inadequate grade of oil | Replace with specified oil
Jumps out of gear | Worn gear shift fork or broken poppet spring | Replace shift fork or poppet spring
Synchronizer hub-to-sleeve spline clearance too large | Replace synchronizer hub and sleeve