| VELOSTER(FS) >2012 > G 1.6 GDI > Engine Mechanical System > General Information>Special Service Tools |

Special Service Tools
Tool (Number and name) | Illustration | Use
Crankshaft front oil seal installer (09455-21200) |  | Installation of the front oil seal
Valve stem oil seal installer (09222-2B100) |  | Installation of the valve stem oil seal
Valve spring compressor and holder A : (09222-3K000) B : (09222-3K100) |  | Removal and installation of the intake or exhaust valve
Crankshaft rear oil seal installer A : (09231-H1100) B : (09231-2B200) |  | Installation of the crankshaft rear oil seal
Ring gear stoppper (09231-2B100) |  | Installation of crankshaft pulley bolt
Engine coolant temperature sensor socket wrench (09221-25100) |  | Removal and installation of engine coolant sensor
Oil pan remover (09215-3C000) |  | Removal of oil pan
Torque angle adapter (09221-4A000) |  | Installation of bolts & nuts needing an angular method