| VELOSTER(FS) >2012 > G 1.6 GDI > Emission Control System > General Information>Components and Components Location |

Components Location
1. PCV valve 2. Canister 3. Purge Control Solenoid Valve (PCSV) 4. Fuel Tank Pressure Sensor (FTPS) | 5. Canister Close Valve (CCV) 6. Fuel Level Sender (FLS) 7. Fuel tank air filter 8. Catalytic converter
1. PCV valve | 2. Canister
3. Purge Control Solenoid Valve (PCSV) | 4. Fuel Tank Pressure Sensor (FTPS)
5. Canister Close Valve (CCV) 7. Fuel tank air filter | 6. Fuel Level Sender (FLS)
8. Catalytic converter (WCC) | 8. Catalytic converter (UCC)