| VELOSTER(FS) >2013 > G 1.6 GDI > Restraint (Advanced) > SRSCM > Front Impact Sensor (FIS)>Description and Operation |

Description
The front impact sensor (FIS) is installed in the front side member. They are remote sensors that detect acceleration due to a collision at its mounting location. The primary purpose of the Front Impact Sensor (FIS) is to provide an indication of a collision. The Front Impact Sensor (FIS) sends acceleration data to the SRSCM.