| VELOSTER(FS) >2013 > G 1.6 GDI > Dual Clutch Transmission(DCT) System>Special Service Tools |

Special tools
Tool (Product number and name) | Shape | Function
09200-38001,09200-3N000 Engine support bar (beam) |  | Remove and install transmission. Supporter (SST No. : 09200-2S100, 2S200) and adapter (SST No. : 09200-4X000) are used together. ※09200-38001 tool can also be used for the task.
09200-2S100 Engine support bar (supporter) |  | Remove and install transmission Beam (SST No. : 09200-38001/3N000), supporter (SST No. : 09200-2S200) and adapter (SST No. : 09200-4X000) are used together.
09200-2S200 Engine support fixture (Supporter) |  | Beam (SST No. : 09200-38001/3N000), supporter (SST No. : 09200-2S100) and adapter (SST No. : 09200-4X000) are used together.
09200-4X000 Engine support bar (adapter) |  | Remove and install transmission Conventional engine support beam (SST No.: 09200-38001,09200-3N000) and supporter (SST No.: 09200-2S000) are used together.
09431-26100 Differential oil seal installer (for housing and case) |  | Install differential oil seal (for housing and case).