| VELOSTER(FS) >2013 > G 1.6 GDI > Engine Electrical System > Cruise Control System>Schematic Diagrams |

System Block Diagram
Component Parts And Function Outline
Component part | Function
Vehicle-speed sensor | Converts vehicle speed to pulse.
ECM | Receives signals from sensor and control switches.
Cruise control indicator | Illuminate when CRUISE main switch is ON (Built into cluster)
Cruise Control switches | ON/OFF switch | Switch for automatic speed control power supply.
Resume/Accel switch | Controls automatic speed control functions by Resume/Accel switch (Set/Coast switch)
Set/Coast switch
Cancel switches | Cancel switch | Sends cancel signals to ECM.
Brake-pedal switch
Transaxle range switch (A/T)
ETS motor | Regulates the throttle valve to the set opening by ECM.
* ETS : Electronic Throttle System